#-------------------------------------------------------------
#########  Printer type setting  ##################################
#Model settings(1:laser;2:CNC;)
>cfg_machine_type:1

#baud rate (9600:1; 57600:2; 115200:3; 250000:4)
>cfg_baud_rate:3

#multi-language(enable:1, disable:0)
>cfg_multiple_language:1

#languages setting(simplified (simplified Chinese:1; traditional Chinese:2; English:3; Russian:4; Spanish:5;French:6;Italian:7).
#This configuration is valid when "cfg_multiple_language" is disabled.
>cfg_language_type:3

#-------------------------------------------------------------
#########  Advanced Function Option  ##################################
#Pause position (-1 is invalid; Z axis is relative position)
>cfg_XPOS:-1
>cfg_YPOS:-1
>cfg_ZADD:10
#enable UPS?(yes:1; no:0)
>cfg_have_ups_device:0

#enable power detecting module(mks 220det:1; mks pwc:0)
>cfg_insert_det_module:0

#enable auto off after print finish function (no:0; Yes:1£©
>cfg_print_finish_close_Machine:0


#---------------------------------------------------------------------------
 
#############  WIFI Function  ##########################################

#wifi model(MKS WIFI TFT:0;  MKS HLK-WIFI:1)
>cfg_wifi_type:0

#wifi mode(AP:1; STA:0)
>cfg_wifi_mode:0

#wifi name and password
>cfg_wifi_ap_name:TP-LINK_C944

>cfg_wifi_key_code:makerbase

#0:disable cloud service 1:enable cloud service
>cfg_cloud_enable:1
#cloud service adress
>cfg_wifi_cloud_host:www.baizhongyun.cn
#cloud service port
>cfg_cloud_port:10086

#Dynamic access IP
>cfg_ip_dhcp_flag:1

#IP/mask/gateway
>cfg_ip_address:192.168.3.100
>cfg_ip_mask:255.255.255.0
>cfg_ip_gate:192.168.3.1

#--------------------------------------------

############## Function Customization #######################################

#command of user-defined function
#>function_btn1_cmd:M84;

#set number of  "More" button  (La version "Laser" du firmware ne permet que 3 boutons...)
>moreitem_pic_cnt:3

#edit command for 1~4 "More" button,each command must be separated by semicolon ";"
# Deplacement de 100 mm en X+ 
>moreitem_button1_cmd:$HX;M03 G91;G0 X100 F3000;
# Deplacement de 200 mm en Y+ 
>moreitem_button2_cmd:M03 G91;G0 Y200 F3000;
# Coup de poinçon
>moreitem_button3_cmd:M03 S1000 G91;G0 F3000;G1 Z1;

#how many "More" button display on screen interface
#>morefunc_cnt:5

#command setting on button1~5
#>morefunc1_cmd:G28;
#>morefunc2_cmd:G28;
#>morefunc3_cmd:G28;
#>morefunc4_cmd:G28;
#>morefunc5_cmd:G28;

#---------------------------------------------
##### Display Customization(button and logo customized see User's Manual) #######

#the color of screen background
>cfg_background_color:0x000000

#the color of title text
>cfg_title_color:0xFFFFFF

#the color of temperature,fan,(etc) background
>cfg_state_background_color:0x000000

#the color of temprature,fan,(etc) text
>cfg_state_text_color:0xFFFFFF

#the color of file button
>cfg_filename_background_color:0x000000

#the color of file text
>cfg_filename_color:0xFFFFFF

#the color of background in printing 
>cfg_printingstat_word_background_color:0x000000

#the color of text in printing status
>cfg_printingstat_word_color:0xFFFFFF

#3D effects setting (disable: 0; enable: 1)
>cfg_BUTTON_3D_effects:0

#Screen rotation 180 ¡ã(0:disable,1:enable)
>cfg_OVERTURN_180:0

#-----------------------------------------------------------------------